ANNEXURE-1

DETAILS OF MACHINES AND EQUIPMENTS

|  |  |  |
| --- | --- | --- |
| S.NO | NAME OF ITEMS/MACHINE | SPECIFICATION |
| 1 | Studio Glass Furnace | Specifications of Equipments for Glass Studio Studio Glass Furnace1. Purpose – Re-melting of Soda-lime Glass
2. Drawing Capacity – 50/70 Kg
3. Holding Capacity – 70/90 Kg
4. Glass Contact Refractory – Mullite
5. Maximum Attainable Temperature –1350/1450oC
6. Temperature Control – Programmable, Fully Automatic
7. Fuel – All Electric
8. Gathering Hole Lid – Hinged
 |
| 2 | Annealing Oven (Programmable) | Annealing Oven (Programmable)1. Inner Dimensions – 900 mm X 600 mm X 600 mm
2. 2 – Tiered
3. All Electric with PID Controller
 |
| 3 | Glory Hole | Glory Hole1. Inner Dimensions – 750 mm x 600 mm ø
2. Dual Door – 450 mm ø / 300 mm ø
3. Gas fired
 |